**DIP CRYSTAL UNITS**

**ZC-M49 Seam Sealing Crystal**

. Very corthpact and thin(7.5\*4.0\*2.3mm MAX)


. Frequency range of 3M～64M with Found

. Low cost ,Wide frequency range,Excellent aging

|  |  |  |
| --- | --- | --- |
| 1 | Nominal Frequency  标称频率 | 3～64MHz |
| 2 | Holding  封装形式 | ZC-M49 |
| 3 | Vibration Mode  振动模式 | AT CUT,FUND/3RD  AT切,基波/三倍波 |
| 4 | Frequency Tolerance @ 25±3℃  调整频差 | ±10PPM /±20PPM/±30PPM |
| 5 | Frequency Stability@ 6  工作温度条件下的频率容差 | ±10PPM /±20PPM/±30PPM |
| 6 | Operating Temperature Range  工作温度 | -20～+70℃/-40～85℃ |
| 7 | Store Temperature Range  存储温度 | -55～+125℃ |
| 8 | Equivalency Resistance  等效电阻 | 20～200Ω max |
| 9 | Load Capacitance  负载电容 | 10～32PF |
| 10 | Drive Level  激励功率 | 100μW max |
| 11 | Insulation Resistance  绝缘阻抗 | ＞500MΩ at DC 100V±15V |
| 12 | Aging  老化 | ±3PPM/year max |

***CRYSTAL CERAMIC DIP 49SS/SMD DIMENSION***

**PACKAGE DIMENSIONS:Unit: mm**



|  |  |  |
| --- | --- | --- |
| NO. | 规格 | H |
| 1. | **F<16Mhz(含)** | **2.3Max** |
| 2 | F>16Mhz | 2.1Max |